Defining Your Needs Clinical Applications Industrial Applications Research Applications Requirements Form Application Note: RCF vs. RPM
| #### Application Note - A Primer on RPM vs. RCF RPM - Stands for revolutions per minute -- the speed you set your centrifuge to spin your rotor. RCF - Stands for relative centrifugal force, also referred to as g-force. The applied force resulting from the spinning action that is perpendicular to the axis of rotation. Force is relative to the earth's gravitational force and has no units, but is simply identified as xg (times gravity) or RCF. g - Stands for gravity. A universal constant that represents the natural pull or force of objects towards the earth. Is there really a difference between RPM and RCF? YES! Since clean sample separation is dependent on the g-force applied, it is important to run at the proper speed that results in your desired g-force. The speed at which you spin your rotor will affect the amount of force applied to your sample. However, the relationship follows this equation RCF = 0.00001118 x radius of rotation (cm) x RPM2 This means that RCF increases exponentially with an increase in RPM. This relationship is shown pictorially below. It assumes that two different rotors are spinning at the same speed of 2500 rpm, however rotor 'A' has a rotating radius of 7.15 cm and rotor 'B' has a rotating radius of 25.75 cm. The resulting g-force at the furthest most point of the tube from the axis of rotation is 500xg and 1800xg respectively. Thus selecting a rotor with a larger radius of rotation will provide higher g-forces at a given speed. Alternately, assume a rotor with a radius of 22.36 cm, running at 4000 rpm results in a RCF of 4000 xg. Changing the speed to 4500 rpm results in a g-force of 5060 xg. To explore this relationship more, experiment with our G-Force Calculator. G-Force Calculator Explained
The G-Force Calculator is provided to aid in your centrifuge selection, because RPM and RCF are not the same. G-force is the driving force behind your separation. The speed at which the rotor spins produces a centrifugal force that follows this relationship, RCF = .00001118 x radius x RPM2 To insure that the centrifuge and rotor you select spins at speeds that achieve g-forces high enough to separate your sample, use the equation above or use our G-Force Calculator. | The G-Force Calculator simplifies this calculation; just enter the speed in rpm and the rotating radius in centimeters, and the g-force calculator will do the math and provide you the RCF, also called g-force. Likewise, enter RCF and radius, and the G-Force Calculator will provide the operating speed in RPM.
| IEC International Equipment Company 300 Second Avenue, Needham Heights, Massachusetts, 02494 USA Phone: 781-449-8060; toll free (USA /Can) 800-843-1113; fax 781-444-6743 Web: http://www.labcentrifuge.com/index.html -- E-mail: info@iec-centrifuge.com Quality .. ISO 9001.. IEC1010-2-020 .. CFC free .. CSA certified .. CE mark .. Safety Copyright © 2000 International Equipment Company. All rights reserved. Home - Centrifuge Products - Applications - Service - About IEC - Contact Us - IEC Worldwide